# spi_master_hw

SPI Master

Author | William Welch Copyright © 2009, all rights reserved.
Adapted-by | Sebastien Lelong
Compiler | 2.4l

Description

    This library has been moved to spi_host_hw due to terminology concerns.

Sources

    good overview of SPI at http://en.wikipedia.org/wiki/Serial_Peripheral_Interface_Bus
    also at: http://elm-chan.org/docs/spi_e.html

Dependencies

- spi_host_hw

## Summary

### Global variables/contants

### Procedures

### Functions

## API details

### Global variables/contants

### Procedures

### Functions

## Related samples

Here are the list of samples which use this library:

16f1823 | 16f1823_nrf905.jal
16f1825 | 16f1825_glcd_ssd1306_font.jal
16f1825 | 16f1825_nrf905.jal
16f1825 | 16f1825_dcf77_decoder_ssd1306.jal
16f18857 | 16f18857_touch_interrupt_ads7843.jal
16f18857 | 16f18857_touch_ads7843.jal
16f18857 | 16f18857_glcd_ili9341_fat32_sd_card.jal
16f18857 | 16f18857_glcd_ssd1306_font_graphics.jal
16f18857 | 16f18857_glcd_ili9341.jal
16f73 | 16f73_temperature_tc77.jal
16f819 | 16f819_mcp2515_can_monitor.jal
16f819 | 16f819_canopen_mcp2515_txhb.jal
16f819 | 16f819_ee25aa02e48_lcd.jal
16f819 | 16f819_mcp2515_canid4_monitor.jal
16f877 | 16f877_fat32_small_pata_hard_disk.jal
16f877 | 16f877_digital_potentiometer_mcp4131.jal
16f877 | 16f877_temperature_tc77.jal
16f877a | 16f877a_digital_potentiometer_mcp4131.jal
16f877a | 16f877a_23k256.jal
16f877a | 16f877a_temperature_tc77.jal
16f877a | 16f877a_fat32_small_pata_hard_disk.jal
16f88 | 16f88_temperature_tc77.jal
18f14k50 | 18f14k50_temperature_tc77.jal
18f2520 | 18f2520_temperature_tc77.jal
18f2550 | 18f2550_temperature_tc77.jal
18f2620 | 18f2620_temperature_tc77.jal
18f452 | 18f452_temperature_tc77.jal
18f452 | 18f452_23k256.jal
18f452 | 18f452_fat32_small_sd_card.jal
18f452 | 18f452_fat32_small_pata_hard_disk.jal
18f452 | 18f452_sd_card.jal
18f452 | 18f452_digital_potentiometer_mcp4131.jal
18f4525 | 18f4525_fat32_sd_card.jal
18f4525 | 18f4525_digital_potentiometer_mcp4131.jal
18f4525 | 18f4525_sd_card.jal
18f4525 | 18f4525_mp3_decoder_vs1053b_sd_card.jal
18f4525 | 18f4525_fat32_small_pata_hard_disk.jal
18f4525 | 18f4525_fat32_pata_hard_disk.jal
18f4525 | 18f4525_mp3_decoder_vs1053b_pata_hard_disk.jal
18f4525 | 18f4525_fat32_small_sd_card.jal
18f4550 | 18f4550_sd_card.jal
18f4550 | 18f4550_digital_potentiometer_mcp4131.jal
18f4550 | 18f4550_fat32_small_sd_card.jal
18f4550 | 18f4550_23k256.jal
18f4550 | 18f4550_temperature_tc77.jal
18f4550 | 18f4550_temperature_max6675.jal
18f4620 | 18f4620_network_webserver_enc28j60.jal
18f4620 | 18f4620_mp3_decoder_vs1053b_sd_card.jal
18f4620 | 18f4620_network_tcp_client.jal
18f4620 | 18f4620_sd_card.jal
18f4620 | 18f4620_temperature_tc77.jal
18f4620 | 18f4620_network_ping.jal
18f4620 | 18f4620_fat32_pata_hard_disk.jal
18f4620 | 18f4620_transceiver_cc1101.jal
18f4620 | 18f4620_network_all_in_one.jal
18f4620 | 18f4620_fat32_small_sd_card.jal
18f4620 | 18f4620_network_tcp_server.jal
18f4620 | 18f4620_network_udp_server.jal
18f4620 | 18f4620_mp3_decoder_vs1053b_pata_hard_disk.jal
18f4620 | 18f4620_network_udp_client.jal
18f4620 | 18f4620_fat32_sd_card.jal
18f4620 | 18f4620_accelerometer_gyroscope_bmi160.jal
18f4620 | 18f4620_digital_potentiometer_mcp4131.jal
18f4620 | 18f4620_fat32_small_pata_hard_disk.jal
18f4620 | 18f4620_quadrature_counter_ls7366r.jal
18f46q10 | 18f46q10_glcd_ili9341_font.jal
18f67j50 | 18f67j50_digital_potentiometer_mcp4131.jal
18f67j50 | 18f67j50_sd_card.jal
18f67j50 | 18f67j50_spi.jal
18f67j50 | 18f67j50_mp3_decoder_vs1053b_sd_card.jal
18f67j50 | 18f67j50_fat32_small_pata_hard_disk.jal
18f67j50 | 18f67j50_fat32_usb_msd_pata_hard_disk.jal
18f67j50 | 18f67j50_fat32_usb_msd_sd_card.jal
18f67j50 | 18f67j50_fat32_pata_hard_disk.jal
18f67j50 | 18f67j50_sd_card_crc.jal
18f67j50 | 18f67j50_mp3_decoder_vs1053b_pata_hard_disk.jal
18f67j50 | 18f67j50_23k256.jal
18f67j50 | 18f67j50_usb_msd_pata_hard_disk.jal
18f67j50 | 18f67j50_usb_msd_sd_card.jal
18f67j50 | 18f67j50_temperature_tc77.jal
18f67j50 | 18f67j50_fat32_sd_card.jal
18f67j50 | 18f67j50_fat32_small_sd_card.jal
18f67j60 | 18f67j60_fat32_sd_card.jal