# reboot

reboot function.

Author | Alun Jones, Copyright © 2012..2012, all rights reserved.
Adapted-by |
Compiler | >=2.4o

Description

    This library provides a single procedure, reboot() which,
    when run, will reboot the PIC. If USB is present, it will disable this
    first and  delay for 2 seconds, which should give any connected master to
    register the disconnect.
    .
    N.B. Does not work on architectures that don't have a reset assembler
    instruction. I've put in a check to report this.

Dependencies

- delay

## Summary

### Global variables/contants

### Procedures

- `reboot()`

### Functions

## API details

### Global variables/contants

### Procedures

- `reboot()`

  No documentation found

### Functions

## Related samples

No sample found