# jascii

ASCII text character constants and case conversion procedures

Author | Wouter van Ooijen, Copyright © 1998, all rights reserved.
Adapted-by | Joep Suijs, Rob Hamerling
Compiler | >=2.4

Description

    - ASCII text character constant definitions
                 - case conversion procedures toupper and tolower

    use of toupper
       var byte char = "b"  -- assign lower case "b" to char
       toupper(char)        -- char now contains "B"

Dependencies

No dependency found

## Summary

### Global variables/contants

- `const byte ASCII_SUB = 26`
- `const byte ASCII_DC4 = 20`
- `const byte ASCII_ETB = 23`
- `const byte ASCII_NAK = 21`
- `const byte ASCII_US = 31`
- `const byte ASCII_SYN = 22`
- `const byte ASCII_RS = 30`
- `const byte ASCII_BS = 08`
- `const byte ASCII_EM = 25`
- `const byte ASCII_EOT = 04`
- `const byte ASCII_DLE = 16`
- `const byte ASCII_LF = 10`
- `const byte ASCII_DC2 = 18`
- `const byte ASCII_ETX = 03`
- `const byte ASCII_ESC = 27`
- `const byte ASCII_CAN = 24`
- `const byte ASCII_SOH = 01`
- `const byte ASCII_ACK = 06`
- `const byte ASCII_HT = 09`
- `const byte ASCII_NULL = 00`
- `const byte ASCII_GS = 29`
- `const byte ASCII_BEL = 07`
- `const byte ASCII_DC1 = 17`
- `const byte ASCII_DC3 = 19`
- `const byte ASCII_SO = 14`
- `const byte ASCII_FF = 12`
- `const byte ASCII_SP = 32`
- `const byte ASCII_ENQ = 05`
- `const byte ASCII_SI = 15`
- `const byte ASCII_CR = 13`
- `const byte ASCII_VT = 11`
- `const byte ASCII_STX = 02`
- `const byte ASCII_DEL = 127`
- `const byte ASCII_FS = 28`

### Procedures

- `toupper(byte in out char)`
- `tolower(byte in out char)`

### Functions

## API details

### Global variables/contants

- `const byte ASCII_SUB = 26`

  No documentation found

- `const byte ASCII_DC4 = 20`

  No documentation found

- `const byte ASCII_ETB = 23`

  No documentation found

- `const byte ASCII_NAK = 21`

  No documentation found

- `const byte ASCII_US = 31`

  No documentation found

- `const byte ASCII_SYN = 22`

  No documentation found

- `const byte ASCII_RS = 30`

  No documentation found

- `const byte ASCII_BS = 08`

  No documentation found

- `const byte ASCII_EM = 25`

  No documentation found

- `const byte ASCII_EOT = 04`

  No documentation found

- `const byte ASCII_DLE = 16`

  No documentation found

- `const byte ASCII_LF = 10`

  No documentation found

- `const byte ASCII_DC2 = 18`

  No documentation found

- `const byte ASCII_ETX = 03`

  No documentation found

- `const byte ASCII_ESC = 27`

  No documentation found

- `const byte ASCII_CAN = 24`

  No documentation found

- `const byte ASCII_SOH = 01`

  No documentation found

- `const byte ASCII_ACK = 06`

  No documentation found

- `const byte ASCII_HT = 09`

  No documentation found

- `const byte ASCII_NULL = 00`

  No documentation found

- `const byte ASCII_GS = 29`

  No documentation found

- `const byte ASCII_BEL = 07`

  No documentation found

- `const byte ASCII_DC1 = 17`

  No documentation found

- `const byte ASCII_DC3 = 19`

  No documentation found

- `const byte ASCII_SO = 14`

  No documentation found

- `const byte ASCII_FF = 12`

  No documentation found

- `const byte ASCII_SP = 32`

  No documentation found

- `const byte ASCII_ENQ = 05`

  No documentation found

- `const byte ASCII_SI = 15`

  No documentation found

- `const byte ASCII_CR = 13`

  No documentation found

- `const byte ASCII_VT = 11`

  No documentation found

- `const byte ASCII_STX = 02`

  No documentation found

- `const byte ASCII_DEL = 127`

  No documentation found

- `const byte ASCII_FS = 28`

  No documentation found

### Procedures

- `toupper(byte in out char)`

      toupper - convert byte to upper case

- `tolower(byte in out char)`

      tolower - convert byte to lower case

### Functions

## Related samples

Here are the list of samples which use this library:

18f27j53 | 18f27j53_sd_card_minix_demo.jal
18f27j53 | 18f27j53_sd_card_minix_readi.jal
18f27j53 | 18f27j53_sd_card_minix_read.jal