# pwm_ccp7

hardware PWM control, dedicated to module PWM7

Author | Stef Mientki, Copyright © 2002-2006, all rights reserved.
Adapted-by | Sebastien Lelong, Rob Hamerling.
Compiler | 2.4p

Description

    Performs PWM operations on the PWM7 module (of enhanced midrange)
    This file is automatically included by pwm_hardware.jal
    when the target PIC has a PWM7 module.

Notes

    1. This is a heavy refactoring of the original pwm_hardware.jal
              (Stef's lib)
           2. Partly rewritten for JalV2 version 2.4l and Jallib revision 1171.
              Reduced memory occupation. Added procedure for lowres PWM.
           3. Changes dd October 2012 by Rob Hamerling
              - added public procedure to set dutycycle with highest resolution (1023 steps).
              - Make the pwm_set_dutycycle (highres, lowres and unqualified) private
                (preceeded with an underscore). These procedures will be kept. but
                with a 'deprecated' warning recommending to use the procedures for
                relative settings.

Dependencies

No dependency found

## Summary

### Global variables/contants

- `var byte _ccpr7l_shadow = 0`
- `var bit*4 _ccp7con_shadow_ccp7m at _ccp7con_shadow : 0`
- `var byte _ccp7con_shadow = 0b0000_0000`
- `var bit*2 _ccp7con_shadow_dc7b at _ccp7con_shadow : 4`

### Procedures

- `pwm7_set_dutycycle(byte in steps)`
- `pwm7_set_dutycycle_lowres(byte in steps)`
- `pwm7_on()`
- `pwm7_set_dutycycle_percent(byte in percent)`
- `pwm7_set_percent_dutycycle(byte in percent)`
- `pwm7_off()`
- `pwm7_set_dutycycle_ratio(word in ratio)`
- `pwm7_set_dutycycle_highres(word in steps)`

Private

- `_pwm7_set_dutycycle_highres(word in steps)`

### Functions

## API details

### Global variables/contants

- `var byte _ccpr7l_shadow = 0`

      8 MSbits of duty cycle

- `var bit*4 _ccp7con_shadow_ccp7m at _ccp7con_shadow : 0`

      2 LSbits of duty cycle

- `var byte _ccp7con_shadow = 0b0000_0000`

      shadow

- `var bit*2 _ccp7con_shadow_dc7b at _ccp7con_shadow : 4`

      2 LSbits of duty cycle

### Procedures

- `pwm7_set_dutycycle(byte in steps)`

      Set dutycycle for 10-bits resolution but allowing only 255 PWM steps.
      This procedure is equivalent to pwm7_set_dutycycle_highres(), but
      the low order 2 bits of the 10-bits duty cycle are set to 0.
      This means that only every 4th of the available 1023 steps can be selected
      and consequently max 255 PWM steps are available.
      This procedure is for user convenience, allowing to specify an 8 bits
      value for the duty cycle is for many applications satisfactory.
      Calling this procedure will also activate PWM.
      Note: pin_CCP7_direction should be set to output!

- `pwm7_set_dutycycle_lowres(byte in steps)`

      Purpose: Set dutycycle with 8-bits resolution allowing 255 PWM steps.
      The 'steps' argument is the 8-bits absolute value for the duty cycle:
      * duty<1:0> are the 2 LSbits
      * duty<7:2> are the 6 MSbits
      Arguments: byte - duty cycle (allowed range 0..255)
      Notes:     This procedure is particularly suitable with higher frequencies
      whereby the PWM resolution is limited to 256 steps or less!

- `pwm7_on()`

      Purpose:   Set PWM on
      Arguments: none
      Notes:     - duty cycle is restored from shadow registers
       pin_PWM7_direction should be set to output

- `pwm7_set_dutycycle_percent(byte in percent)`

      Purpose:   Set duty cycle as a percentage, allowing max 100 PWM steps.
      The duty cycle will be set to the specified percentage of the maximum
      for the current PWM frequency and Fosc.
      Arguments: byte - dutycycle as a percentage (allowed range: 0..100)
      Notes:     - The number of available PWM steps can be lower than 100 with
      (very) high PWM frequencies and low Fosc.
       The steps may not all be equal. The lower the actual resolution
      the bigger the differences between steps may be.
       pin_CCP7_direction should be set to output!

- `pwm7_set_percent_dutycycle(byte in percent)`

      deprecated procedure

- `pwm7_off()`

      Purpose:   PWM mode off
      Arguments: none

- `pwm7_set_dutycycle_ratio(word in ratio)`

      Purpose:   Set duty cycle in the range 0..1023 PWM steps.
      Arguments: word - dutycycle ration in range 0..1023
      Notes:     - The duty cycle will be set to the specified ration of the maximum
      value for the current PWM frequency and Fosc.
      Notes:     - The resolution is about 1 pro mille
       The number of available PWM steps can be lower than 1023 with
      high PWM frequencies or low Fosc values.
       pin_CCP7_direction should be set to output!

- `pwm7_set_dutycycle_highres(word in steps)`

      deprecated procedure

Private

- `_pwm7_set_dutycycle_highres(word in steps)`

      Purpose:   Specify the duty cycle by number of PWM steps.
      The duty cycle is setting is determined by a 10-bits parameter,
      allowing a resolution of 1023 steps.
      The 'steps' argument is a (max) 10-bits absolute value for the duty cycle:
      * steps<1:0> are the 2 LSbits
      * steps<9:2> are the 8 MSbits
      Arguments: word - steps cycle (allowed range 0..1023)
      Notes:     - This is a private procedure, not intended for general use.
      The caller is responsible to specify an acceptable value
      w.r.t. to the chosen PWM frequency.

### Functions

## Related samples

No sample found