# max7219_font

Fonts for MAX7219 seven segment library

Author | Rob Hamerling, Copyright © 2014..2014, all rights reserved.
Adapted-by |
Compiler | 2.4q3

Description

    Fonts for MAX7219 7-segment displays.
    Only a (hexa)numeric font is supported (chars 0123456789abcdef).
    The MAX7219 has a 'reversed' bit representation of the segments
    than usual (compared to TM1638/40 and others), see the mapping below:
    .
       -- 6 --
      |       |
      1       5
      |       |
       -- 0 --
      |       |
      2       4
      |       |
       -- 3 --  .7

Dependencies

No dependency found

## Summary

### Global variables/contants

- `const byte _MAX7219_MINUS = 0b00000001`
- `const byte _MAX7219_NUMBER_FONT[] = { 0b01111110,`

### Procedures

### Functions

## API details

### Global variables/contants

- `const byte _MAX7219_MINUS = 0b00000001`

      minus / hyphen

- `const byte _MAX7219_NUMBER_FONT[] = { 0b01111110,`

      definition for standard (hexa)decimal numbers

### Procedures

### Functions

## Related samples

No sample found