# large_array_2

Large Array_2 library

Author | Oliver "Kiste" Seitz, copyright © 2009..2020, all rights reserved.
Adapted-by |
Compiler | >=2.5r6

Description

    This library is for creating an array that take up more than one
                 GPR segment of memory. Works for PIC14(H) and PIC16 cores. It is
                 a complete rewrite of the original large_array_2 lib.

Sources

    This file is generated by script: generate_large_array.py

Notes

    For controllers with PIC16 core (labeled PIC18(l)f...)
    Supports byte array with up to 14848 entries (LARGE_ARRAY_1_VARIABLE_SIZE = 1)
    Supports word array with up to 7424 entries (LARGE_ARRAY_1_VARIABLE_SIZE = 2)
    Supports dword array with up to 3712 entries (LARGE_ARRAY_1_VARIABLE_SIZE = 4)

Dependencies

No dependency found

## Summary

### Global variables/contants

### Procedures

### Functions

## API details

### Global variables/contants

### Procedures

### Functions

## Related samples

Here are the list of samples which use this library:

16f1825 | 16f1825_large_array.jal
16f18857 | 16f18857_glcd_ili9341_fat32_sd_card.jal
18f26j50 | 18f26j50_fat32_sd_card.jal
18f4525 | 18f4525_mp3_decoder_vs1053b_pata_hard_disk.jal
18f4525 | 18f4525_fat32_sd_card.jal
18f4525 | 18f4525_mp3_decoder_vs1053b_sd_card.jal
18f4525 | 18f4525_fat32_pata_hard_disk.jal
18f4620 | 18f4620_mp3_decoder_vs1053b_pata_hard_disk.jal
18f4620 | 18f4620_mp3_decoder_vs1053b_sd_card.jal
18f4620 | 18f4620_fat32_sd_card.jal
18f4620 | 18f4620_fat32_pata_hard_disk.jal
18f67j50 | 18f67j50_fat32_pata_hard_disk.jal
18f67j50 | 18f67j50_fat32_sd_card.jal
18f67j50 | 18f67j50_fat32_usb_msd_pata_hard_disk.jal
18f67j50 | 18f67j50_mp3_decoder_vs1053b_pata_hard_disk.jal
18f67j50 | 18f67j50_mp3_decoder_vs1053b_sd_card.jal
18f67j50 | 18f67j50_fat32_usb_msd_sd_card.jal
18f67j60 | 18f67j60_fat32_sd_card.jal