# glcd_6x8_font

6X8 font lookup table for GLCD with pcd8544 controller used in Nokia 3310

Author | Richard Zengerink Copyright © 2008..2022, all rights reserved.
Adapted-by | Rob Jansen
Compiler | 2.5r6

Description

    library 6X8 font lookup table for Nokia 3310 display with pcd8544 controller

Sources

    http://www.amontec.com/lcd_nokia_3310.shtml

Notes

    See lib glcd_font.jal for font explanation

Dependencies

No dependency found

## Summary

### Global variables/contants

- `const byte FONT_6X8_CHARS[] =`
- `const byte FONT_6X8_WIDTH = 6`
- `const byte FONT_6X8_BYTE_PER_CHAR = 6`
- `const byte FONT_6X8_BIT_DIRECTION = FONT_BOTTOM_LEFT_VERTICAL`
- `const byte FONT_6X8 = 0x05`
- `const byte FONT_6X8_HEIGHT = 8`

### Procedures

### Functions

## API details

### Global variables/contants

- `const byte FONT_6X8_CHARS[] =`

      6X8, BOTTOM_LEFT, VERTICAL, NO_NAME

- `const byte FONT_6X8_WIDTH = 6`

  No documentation found

- `const byte FONT_6X8_BYTE_PER_CHAR = 6`

  No documentation found

- `const byte FONT_6X8_BIT_DIRECTION = FONT_BOTTOM_LEFT_VERTICAL`

  No documentation found

- `const byte FONT_6X8 = 0x05`

      Font ID, unique amongst font libs.

- `const byte FONT_6X8_HEIGHT = 8`

  No documentation found

### Procedures

### Functions

## Related samples

Here are the list of samples which use this library:

16f1825 | 16f1825_dcf77_decoder_ssd1306.jal
16f1825 | 16f1825_gps_neo_6m_ssd1306_clock.jal
16f1825 | 16f1825_nec_rc_decoder_ssd1306.jal
16f1825 | 16f1825_philips_rc_decoder_ssd1306.jal
16f1825 | 16f1825_glcd_ssd1306_font.jal
16f1829 | 16f1829_glcd_ks0108.jal
16f18857 | 16f18857_glcd_ssd1306_font_graphics.jal
18f4550 | 18f4550_glcd_nokia_5110_font.jal
18f46q10 | 18f46q10_glcd_ili9341_font.jal
18f6310 | 18f6310_glcd_ks0108.jal
18f6310 | 18f6310_glcd_ks0108_math.jal