# temperature_max6675

Library for max6675 Temperature for K-Thermocouple with SPI.

Author | Matthew Schinkel - borntechi.com, copyright © 2009, all rights reserved.
Adapted-by |
Compiler | >=2.4q2

Description

    Library for max6675 Temperature IC to convert a
                 Cold-Junction-Compensated K-Thermocouple to a
                 Digital reading (0C to +1024C).

Sources

    http://datasheets.maximintegrated.com/en/ds/MAX6675.pdf

Dependencies

- delay

## Summary

### Global variables/contants

### Procedures

### Functions

- `max6675_temp_c() return word`
- `max6675_temp_f() return word`

## API details

### Global variables/contants

### Procedures

### Functions

- `max6675_temp_c() return word`

      Returns Celsius

- `max6675_temp_f() return word`

      Returns Fahrenheit

## Related samples

Here are the list of samples which use this library:

18f4550 | 18f4550_temperature_max6675.jal