# glcd_90x90_jal_logo

JAL bitmap image array generated from an RGB565 bitmap file.

Author | Script by Rob Jansen, Copyright © 2022..2022, all rights reserved.
Adapted-by |
Compiler | 2.5r6

Description

    An RGB565 bitmap image converted to JAL Array.

Notes

    A way to generate the RGB565 bitmap from a png or jpg file:
                 Converter: https://online-converting.com/image/convert2bmp/
                 Choose: 16 (5:6:5 RGB Hi-Color), rows direction Top - Bottom

Dependencies

No dependency found

## Summary

### Global variables/contants

- `const word JAL_LOGO_BITMAP[JAL_LOGO_WIDTH * JAL_LOGO_HEIGHT] =`
- `const word JAL_LOGO_WIDTH = 90`
- `const word JAL_LOGO_HEIGHT = 90`

### Procedures

### Functions

## API details

### Global variables/contants

- `const word JAL_LOGO_BITMAP[JAL_LOGO_WIDTH * JAL_LOGO_HEIGHT] =`

      Bitmap image.

- `const word JAL_LOGO_WIDTH = 90`

      Image size.

- `const word JAL_LOGO_HEIGHT = 90`

  No documentation found

### Procedures

### Functions

## Related samples

Here are the list of samples which use this library:

16f18857 | 16f18857_glcd_ili9341.jal