# glcd_5x7_font

5X7 font lookup table for GLCD with pcd8544 controller used in Nokia 3310

Author | Andre Miller Copyright © 2008..2022, all rights reserved.
Adapted-by | Richard Zengerink, Rob Jansen
Compiler | 2.5r6

Description

    library 5X7 font lookup table for Nokia 3310 display with pcd8544 controller

Sources

    http://www.amontec.com/lcd_nokia_3310.shtml

Notes

    See lib glcd_font.jal for font explanation

Dependencies

No dependency found

## Summary

### Global variables/contants

- `const byte FONT_5X7_CHARS[] =`
- `const byte FONT_5X7_BYTE_PER_CHAR = 5`
- `const byte FONT_5X7_WIDTH = 5`
- `const byte FONT_5X7_BIT_DIRECTION = FONT_BOTTOM_LEFT_VERTICAL`
- `const byte FONT_5X7 = 0x02`
- `const byte FONT_5X7_HEIGHT = 7`

### Procedures

### Functions

## API details

### Global variables/contants

- `const byte FONT_5X7_CHARS[] =`

      5X7, TOP_LEFT, HORIZONTAL, NO_NAME

- `const byte FONT_5X7_BYTE_PER_CHAR = 5`

  No documentation found

- `const byte FONT_5X7_WIDTH = 5`

  No documentation found

- `const byte FONT_5X7_BIT_DIRECTION = FONT_BOTTOM_LEFT_VERTICAL`

  No documentation found

- `const byte FONT_5X7 = 0x02`

      font ID, unique amongst font libs

- `const byte FONT_5X7_HEIGHT = 7`

  No documentation found

### Procedures

### Functions

## Related samples

Here are the list of samples which use this library:

16f1825 | 16f1825_glcd_ssd1306_font.jal
16f18857 | 16f18857_glcd_ssd1306_font_graphics.jal
16f877a | 16f877a_glcd_ks0108.jal
18f2580 | 18f2580_rtc_ds1302_glcd.jal
18f4550 | 18f4550_glcd_nokia_5110_image.jal
18f4550 | 18f4550_glcd_nokia_5110_gfx.jal
18f4550 | 18f4550_glcd_nokia_5110_pixel.jal
18f4550 | 18f4550_glcd_nokia_5110_sprite.jal
18f4550 | 18f4550_glcd_nokia_5110_font.jal
18f46q10 | 18f46q10_glcd_ili9341_font.jal